# Analyte Flux and Load from Estimates of Concentration and Discharge

## Documentation for package ‘realTimeloads’ version 1.0.0

- DESCRIPTION file.
- User guides, package vignettes and other documentation.
- Package NEWS.

## Help Pages

acoustic_backscatter_processing | Process acoustic backscatter from hADCP
attenuation_of_sound_by_water | Compute attenuation of sound in water given frequency, temperature, and salinity
bootstrap_regression | Regression parameters estimated using bootstrap resampling
butterworth_tidal_filter | Return non-tidal signal in data after Rulh and Simpson (2005)
compute_load | Compute load with uncertainty on concentration estimates
ctd2sal | Compute salinity (PSU) from conductivity, water temperature, and depth
estimate_timeseries | Compute timeseries with uncertainty from bootstrap regression
ExampleCode | Computes sediment load per guideline from ExampleData
ExampleCodeSCI | Computes sediment load from optical and acoustic backscatter measurements
ExampleData | Example data used to demonstrate computation of real-time sediment loads from horizontal acoustic Doppler current profiler (hADCP)
hADCPLoads | Compute sediment load per guideline using acoustic backscatter from processed hADCP data
import_data | Load data from comma-delimited .txt files to list to be used in function hADCPLoads()
impute_data | Returns x with gaps imputed using ARIMA and Decision Trees, optional uncertainty estimation using Monte Carlo resampling
linear_interpolation_with_time_limit | Linearly interpolate timeseries time(x) onto new timesetep ti
near_field_correction | Near-field correction of Downing et al (1995)
speed_of_sound | Compute speed of sound in water given salinity, temperature, and depth
surrogate_to_analyte_interpolation | Interpolate timeseries x(tx) onto y(ty)