# Urban Environment Analysis Using Global Building Height Datasets

## Documentation for package ‘gloBFPr’ version 2.0.0

- DESCRIPTION file.
- User guides, package vignettes and other documentation.

## Help Pages

add_flow_vectors | Add wind / flow vector arrows to a foam map plot
aggregate_block | aggregate_block
generate_block | generate_block
get_3d_world | get_3d_world
get_bgvi | get_metrics
get_dng | get_metrics
get_era5_met | Fetch ERA5 conditions for OpenFOAM boundary conditions
get_fused_dsm | get_fused_dsm
get_metadata | get_metadata
get_metrics | get_metrics
get_morphology | get_metrics
get_neighbors | get_metrics
get_noise_map | Create a screening-level urban road-noise workflow object
get_radiation | Building shadow and radiation calculations
get_shadows | Building shadow and radiation calculations
get_shadow_footprint | Building shadow and radiation calculations
get_shadow_height | Building shadow and radiation calculations
globfp_example | Test 3D-GloBFP dataset
globfp_example_canopy_height | Example canopy height raster for the 3D-GloBFP sample
globfp_example_dem | Example DEM for the 3D-GloBFP sample
infer_osm_traffic | Infer screening-level road traffic inputs from OSM road attributes
install_noisemodelling | Install the headless NoiseModelling runner
osm_noise_traffic_defaults | Default OSM traffic assumptions for screening-level road noise
plot_bgvi_viewshed | Visualize an Individual Building BGVI Viewshed
plot_foam_map | Plot an OpenFOAM pedestrian-level map
plot_noise_map | Plot a NoiseModelling-style road-noise map
prepare_foam_case | Prepare a transient OpenFOAM case for urban wind
prepare_foam_geometry | Build terrain, canopy and terrain-based building geometry for a case
prepare_noisemodelling_inputs | Prepare NoiseModelling-style input layers
prepare_openfoam_inputs | Prepare gloBFPr spatial outputs for an OpenFOAM Docker workflow
read_foam_pedestrian_slice | Read the pedestrian-level slice and compute wind maps
run_openfoam_docker | Run an OpenFOAM case via Docker
sample_foam_slice | Sample OpenFOAM results at pedestrian level and return a raster
search_3dglobdf | search_3dglobdf
svf | Building shadow and radiation calculations